TAPI for snom Help:
Extended settings

- TAPI for snom Phones
- Installation
- Configuration Pages

- Connection
- Dial
- Action URLs

- Firewall Configuration

- Extended settings

- FAQ

#### Detect Special States

> Timeout for incoming calls | For calls from a call group, the phone may not report an end of call (IDLE) via Action URL. To prevent the call from ringing forever, a maximum value (in seconds) can be specified after the driver itself generates an IDLE.
> "Hang Up" after redirect incoming call | The snom log file is analysed to detect the hangup state of your snom phone after you have redirected an incoming call.
> Disconnect a call on hold | If a "Disconnect" is received, the SIP.log from Snom phone is analyzed to determine whether the active or held call has been disconnected.