TAPI for snom Help:
Dial

- TAPI for snom Phones
- Installation
- Configuration Pages

- Connection
- Dial
- Action URLs

- Firewall Configuration

- Extended settings

- FAQ

#### Identity for Outgoing Calls

> If you have entered multiple identities in your phone you can select one for outgoing calls:

> - via phone configuration or
> - via TAPI application (temporary)

#### TAPI Functions

> Pickup: Enter here your telephone system pickup code, eg '* 77'. Please ask your administrator or telephony provider for the required pickup code.
> The check mark at "+ number" should normally be set. The option causes the pickup code is automatically extended and executed with the destination number.

#### Global Settings

> Dial Timeout: If no information about dialing is received from the phone, then an IDLE will be generated for the TAPI-Call after "Timeout" seconds.

> CSTA-Dial: If the TAPI dialing does not work for numbers starting with #, you can alternatively activate this dialing mode.