TAPI for snom Help:
Installation

- TAPI for snom Phones
- Installation

- Test with Outlook or phone.exe

- Configuration Pages
- FAQ

On this page

- 1. Download and Installation
- 2. TAPI Driver Configuration
- 2.1. Configure Telephone IP
- 2.2. Configure Actions URLs
- 3. Hints for Administrators

How to set-up xtelsio TAPI for snom:

#### 1. Download and Installation

> 1. Download und extract xtelsio_TAPI_for_snom_setup.zip.
> 2. Run setup.exe and follow the dialogs.
>    You will need Administator rights.

#### 2. TAPI Driver Configuration

> You can open the driver configuration via: [Start > Programs > xtelsio_TAPI_for_snom > xtelsio TAPI for snom - Configuration > Configure...].

> | xtelsio TAPI for snom - Configuration
> | snom Line1

> To configure the TAPI line, use the lower button [Settings...].
> => Configuration Pages

> Hints:

> - The button [Delete] can be used only for the last TAPI Line.
> - The state "closed" means only that the TAPI Line was currently not open by any TAPI application.

#### 2.1. Configure Telephone IP

> Configure the Phone IP address in the dialog [Connection].

#### 2.2. Configure Actions URLs

> Configure the Phone IP address in the dialog [Connection].

> Configure the Actions URLs in dialog [Actions URL].
> The Actions URLs are needed to detect and display incoming and outgoing calls.

> Hint: If the Actions URLs do not work, no incoming calls are displayed.

> If these settings are done the TAPI driver should work now.

> Test with Outlook

#### 3. Hints for Administrators

> Terminal Server Installation