TAPI for snom Help:
Connection

- TAPI for snom Phones
- Installation
- Configuration Pages

- Connection
- Dial
- Action URLs

- Firewall Configuration

- Extended settings

- FAQ

#### Connection Settings

> | TAPI for snom - Line Configuration

> IP Address | = IP address of the phone
> Port | = HTTP port for telephone web configuration; default=80
> Authentication, Username, Password | If you enter the IP address of your phone into web browser, a username and password my be queried. The same credentials are entered here.
> Test | If the test indicates an error, please check the connection parameters in your web browser. Enter the IP address of your phone in web browser. Unter Citrix gab es auch schon Probleme, wenn die "MTU Size" auf 1500 statt auf 1300 stand.

> ##### More information

> - DECT phones are not supported.
> - Please check also whether the correct local IP address of your computer is selected on the tab "Action URLs" or "Local IP".
> - The display of "supported models" is for information only and has no functional effect.