2.2 | Starting installation

Starting installation

1. | Log on as an administrator and close all running applications.

2. | Insert the TAPI 120 installation CD. Select Start - Run, enter the file \TAPI120\setup.exe on the installation drive and confirm with OK.

The setup determines the operation system version (32-bit or 64-bit) and automatically starts the installation of the correct TAPI 120 setup version.

3. | Confirm the UAC (User Account Control) prompt.

4. | Select the language for the installation dialogs, the installation is prepared.

5. | After installation preparation the welcome-Dialog appears. Confirm it with Next.

Make sure, that the service-control dialog and all TAPI applications are inactive. Corresponding to this a red marked notice appears in the installation dialog.

6. | Continue installation with clicking Next.

7. | The installation setup type must then be specified:

Display

8. | Select the components to be installed in the dialog displayed and confirm with Next.

9. | Installation of the selected components is started after clicking Install.

The initial installation of TAPI 120 on a PC with Windows 10/8.1/8/7 or Windows Vista requires a reboot of the TAPI-PC. In that case the installation dialog displays an additional red marked notice.
You then can cancel the installation. For continuing the installation you click on Install, the PC automatically reboots. After logging on you return to this point of the TAPI 120 installation procedure.

| - | Installing the CMD component

| - | Installing the TSP component

10. | To finish installation click on the Finish button displayed in the final dialog.