3.2.2 | General parameters

For configuring basic settings and the setup connection parameters to your OpenScape Business system select the UC-Server tab.

Depending on the selected operation mode the number and type of settings change.

Display (operation mode OpenScape Business TAPI CSTA)

Display (Operation mode OpenScape Business UC Smart)

The parameters in the UC-Server tab contain the following information:

Parameter
Description
Operation mode
Available Operation modes are:
• | OpenScape Business TAPI CSTA Your OpenScape Business system is connected via the available CSTA interface (Booster Card / Booster Server or integrated).
• | OpenScape Business TAPI UC Smart Your OpenScape Business basic system is connected via the WSI interface.
IP address of your Server
IP address of the system determined during its installation and configuration of OpenScape Business.
• | In operation mode OpenScape Business TAPI CSTA this is the IP address of the Booster Card / Booster Server / Business S).
• | In operation mode OpenScape Business TAPI UC Smart this is the IP address of the OpenScape Business system (X1 / X3 / X5 / X8).
IP port of the Server
IP port number of the OpenScape Business system.
• | In operation mode OpenScape Business TAPI CSTA this is 8900 by default.
• | In operation mode OpenScape Business TAPI UC Smart the IP port is displayed subject to the selected Protocol to Server. The IP port is 8802 for secure connection (HTTPS) and 8801 for unsecure connection (HTTP).
Protocol to Server
In OpenScape Business TAPI UC Smart operation mode you configure this settings for the server protocol:
• | Transfer protocol for the TAPI 120 connection to the system. You can select HTTP (unsecure connection) or by default HTTPS (secure connection). This option has to correspond with the setting on the system.
• | If HTTPS certificate prompts (e.g. when using a self-signed certificate) should be automatically ignored, activate the Ignore certificate errors option.
UC Smart User
In OpenScape Business TAPI UC Smart operation mode you enter the UC Smart user.
Extension number
In OpenScape Business TAPI CSTA operation mode enter the Extension of the telephone to be controlled.
TAPI Line-name/description
For a better identification of the TAPI 120 line in the application you enter a TAPI Line-name or a description here.
UC Smart Password
In OpenScape Business TAPI UC Smart operation mode you enter the password assigned to the UC Smart User.
UC Smart user informations can be edited in the UC Smart Assistant. Click on the Click here to open UC Smart Assistant for starting the Assistant.
You find more information about UC Smart Assistant in the myPortal documentation.

Saving parameters

> | Click Apply to save entries without closing the dialog. e.g. to configure parameters in other tabs.
> | Click OK to save changes and to exit the configuration dialog.
> | A confirmation message appears in both cases. Click Yes to confirm this message. Changes take effect after a Telephony service restart on the TAPI PC.

Operation mode TAPI CSTA: Connection test between TAPI 120 and the system

Immediately after installation of TAPI 120 Windows does not know the TAPI 120 user (TAPI Line-name/description). Therefore in the TAPI 120 configuration dialog the button Test Connection is not shown during the initial installation of TAPI 120.

After entering the Extension number respectively the TAPI Line-name/description of the telephone to be controlled you can test the connection of TAPI 120 to this Extension number with click on Test connection. The tests result is displayed in a info box:

| - | Connection OK Between TAPI 120 and the system the connection can be established, the licensing of the extension is correct, TAPI 120 is ready.

| - | Please check the TAPI License for this subscriber! Between TAPI 120 and the system the connection can be established, the licensing of the extension is not correct, TAPI 120 is not ready.

| - | CTI Firewall Ok, but unspecified error at startMonitor! Between TAPI 120 and the system the connection can be established, the extension / name is identified on the system but can not be activated, TAPI 120 is not ready.

| - | Used subscriber not known by the system! Between TAPI 120 and the system the connection can be established, the extension / name is not configured on the system. TAPI 120 is not ready.

| - | Please check the CTI firewall! Between TAPI 120 and the system no connection can be established. The CTI firewall of OpenScape Business rejects this users login (possibly the automatic registration is inactive). TAPI 120 is not ready.

| - | Please check the connection settings! The system is not accessible in the network. This can originate from general network problems, an inactive system / inactive CSTA link, an invalid IP address / IP port if the system, etc.