3 | Configuring TAPI 120

3.1 | General

Configuration dialog

The individual TAPI 120 configuration can be done in the configuration dialog started during the installation automatically or at a later point in time.

Effectiveness of modified configuration parameters

Modified configuration parameters are saved with clicking Apply or OK in the configuration dialog. The modification will be effective once the Telephony service on the TAPI PC has been restarted.