2 | Installation of TAPI 120

2.1 | Starting the installation

1. | Log on as an administrator and close all running applications.

2. | Insert the TAPI 120 installation CD labeled OpenScape Business TAPI 120/170 Service Provider.

3. | Select Start - Run, enter the file \TAPI120\setup.exe on the installation drive and confirm with OK.

The setup determines the operation system version (32-bit or 64-bit) and automatically starts the installation of the correct TAPI 120 setup version.

Confirm the UAC (User Account Control) prompt that appears during installation now.

4. | Select the language for the installation dialogs, the installation is resuming.

5. | After installation preparation the welcome dialog appears. Confirm it with Next.

Make sure, that the service-control dialog and all TAPI applications are inactive. Corresponding to this a red marked notice appears in the installation dialog.

6. | Continue installation with clicking Install.

The initial installation of TAPI 120 requires a restart of the TAPI-PC. In that case the installation dialog displays an additional red marked notice.
You then can cancel the installation. For continuing the installation you click on Install, the PC automatically reboots. After logging on you automatically return to this point of the TAPI 120 installation procedure.

7. | Installation is started, installation progress will be shown.

8. | To finish installation click on the Finish button displayed in the final dialog.

9. | The TAPI 120 configuration dialog opens automatically after the successful installation. The required parameters can be entered in this dialog or configured at a later stage.

Display

| Each configuration parameter is described under Configuration of TAPI 120.

| The TAPI 120 installation is complete once you have exited the configuration dialog.